
**Numark Orbit – Remix Deck Mapping**

*This mapping requires Traktor Pro 2.6.2 or higher*

1. Plug in and power on your Numark Orbit.
2. Open **Numark Orbit Editor**. If you do not have the Orbit MIDI Editor you can download it [here](http://www.numark.com/ozone).
3. Click **Load** from the **Manage Mappings** section.  
     
   
4. Browse your computer to locate the **Orbit Remix Deck MIDI Preset.json** editor file.
5. Click **Send**. You should see **Mapping Sent Successfully**.
6. **Close** Numark Orbit Editorby clicking **File** >**Exit** (Windows) or **Quit** Numark Orbit Editorfrom top menu(Mac).
7. Open Traktor Pro 2.6.2 Software.
8. Click the **Preferences** or **gear** icon from the top right menu.   
     
   
9. Select **Controller Manager** from the list on the left.
10. Click the **Add… > Import** from **Device Setup**.   
      
    
11. Browse your computer to locate the Windows or Mac **Orbit Remix Deck [C] or [D].tsi** mapping file.
12. Ensure that the **Numark Orbit** is selected as your **In-Port**, and **Out-Port**.  
      
    

