**Numark MIXDECK QUAD - 4 Deck Mapping for Traktor Pro**  
 *\*This Mapping requires Traktor Pro 2.6 or higher.*

**Mapping Highlights**




* 4 Deck Control - Bleep/Reverse Toggles Deck.
* New Traktor Pro 2.6 Features - Flux Mode, Auto-Gain, Macro FX.
* Full FX Control - Deck A/C (Unit 1), Deck B/D (Unit 2).

**Mapping Setup**

1. Download the mapping.
2. Unzip the file.
3. Open Traktor Pro 2.6+ Software.
4. Click the Preferences icon from the top right menu.
5. Click the Import button from the bottom of the Preferences window.
6. Select the mapping MIXDECK QUAD .tsi file
7. Make sure all of the boxes a checked like below.   
     
   
8. Repeat this step **TWICE** to ensure the settings load correctly.

**Audio Setup**

By default when you import the mapping file with the **Audio Device Settings** box checked the setup should be automatic. If you have any troubles at all make sure your settings match the settings below.

1. Set the **USB AUDIO** switch on the rear of the unit to **PGM/CUE**.
2. Click on the **Preferences** icon in the top right corner.  
     
   
3. Click on the **Audio Setup** tab on the left side.
4. Set the **Audio Device** to **MIXDECK QUAD**.  
     
   
5. Click on the **Output Routing** tab on the left side.
6. Set the **Output Monitor**, and **Output Master** to mirror the settings below.   
      
   **Mac**  
     
   **Windows**   
   
7. Close the **Preferences** window.

**Button Layout**

