**Numark 4TRAK FX Bar LED Fix**

1. Unzip the files.
2. Open Traktor Pro 2.
3. Open Preferences.
4. Select Controller Manager on the left.
5. Delete existing FX Bar mapping.
6. Edit... > Delete.
7. Click Add... > Import.
8. Select the Numark\_4TRAK\_FX\_Bar\_LED\_Fix.tsi (Windows or Mac).
9. Set 4TRAK-FX as the In-Port and Out-Port. (Should automatically set).