**Numark NV Firmware Update Instructions**

Please read these instructions carefully.  \*\*This v1.06 update is not a new firmware update.  If you didn’t experience any error messages displayed on your NV screens, please don’t update to this current firmware.  This update will rectify the following error messages that are displayed on your NV screens:

ERROR 12: Application Missing.  Run Firmware Update Mode – O

ERROR 3: invalid MMA2. Run firmware Update Mode – 2

ERROR 2: invalid MMA1 Run Firmware Update Mode - 1

Boot Loader Init

1. Download the firmware updater.
2. Connect NV to computer powered on.
3. Run the attached updater app.
4. Click “Update Firmware”.
5. Please follow the on-screen instructions exactly as they appear.
6. Power off when prompted to on-screen.
7. Hold down the PLAY and CUE buttons on the left deck while powering on the unit.
8. Press the blinking PLAY button.
9. At this time, the firmware will be erased on both screens. This may take several minutes.  Once complete you will be prompted to hit the OK button to start the update process.

Do not unplug or power off the unit during this time.

Once the update is complete, power the unit off, wait 5 seconds, power on and enjoy.